27/03/2025 13:47:10 : Created file: C:\Users\promerogomb\Desktop\fluxcontrol\motores\PLACond\MessageLogs\messageLog_14884.txt
27/03/2025 13:47:10 : Loaded file: C:\Users\promerogomb\Desktop\fluxcontrol\motores\PLACond.mot
27/03/2025 13:47:11 : pymotorcad: ShowMagneticContext
27/03/2025 13:47:11 : pymotorcad: SetVariable ShaftSpeed = 3000
27/03/2025 13:47:11 : pymotorcad: SetVariable CurrentDefinition = 1
27/03/2025 13:47:11 : pymotorcad: SetVariable RMSCurrent = 3
27/03/2025 13:47:11 : pymotorcad: SetVariable DCBusVoltage = 350
27/03/2025 13:47:11 : pymotorcad: SetVariable PhaseAdvance = 45
27/03/2025 13:47:11 : pymotorcad: SetVariable MagneticThermalCoupling = 0
27/03/2025 13:47:11 : pymotorcad: SetVariable BackEMFCalculation = False
27/03/2025 13:47:11 : pymotorcad: SetVariable CoggingTorqueCalculation = False
27/03/2025 13:47:11 : pymotorcad: SetVariable ElectromagneticForcesCalc_OC = False
27/03/2025 13:47:11 : pymotorcad: SetVariable TorqueSpeedCalculation = False
27/03/2025 13:47:11 : pymotorcad: SetVariable DemagnetizationCalc = False
27/03/2025 13:47:11 : pymotorcad: SetVariable ElectromagneticForcesCalc_Load = False
27/03/2025 13:47:11 : pymotorcad: SetVariable InductanceCalc = False
27/03/2025 13:47:11 : pymotorcad: SetVariable BPMShortCircuitCalc = False
27/03/2025 13:47:11 : pymotorcad: SetVariable TorqueCalculation = True
27/03/2025 13:47:11 : pymotorcad: GetVariable SHAFTSPEED = 3000
27/03/2025 13:47:11 : pymotorcad: GetVariable CURRENTDEFINITION = 1
27/03/2025 13:47:11 : pymotorcad: GetVariable PEAKCURRENT = 4,24264068711929
27/03/2025 13:47:11 : pymotorcad: GetVariable TORQUECALCULATION = True
27/03/2025 13:47:11 : pymotorcad: DoMagneticCalculation
27/03/2025 13:47:12 : Creating folder: C:\Users\promerogomb\Desktop\fluxcontrol\motores\PLACond\FEResultsData\
27/03/2025 13:47:12 : Creating folder: C:\Users\promerogomb\Desktop\fluxcontrol\motores\PLACond\FEResultsData\feasys\
27/03/2025 13:47:12 : Status: Solving FEA model
27/03/2025 13:47:13 : Q axis current only Point Calculation
27/03/2025 13:47:13 : Solving FEA model
27/03/2025 13:47:13 : Load Point Calculation
27/03/2025 13:47:13 : Solving FEA model
27/03/2025 13:47:14 : Solving FEA model
27/03/2025 13:47:14 : Transient Torque Calculation
27/03/2025 13:47:14 : Solving FEA model
27/03/2025 13:47:23 : FEA Calculation Time: 10 Seconds
27/03/2025 13:47:23 : Creating folder: C:\Users\promerogomb\Desktop\fluxcontrol\motores\PLACond\FEResultsData\feasys\
27/03/2025 13:47:23 : Warning: Operating point outside voltage limit. Check the DC bus voltage.
27/03/2025 13:47:23 : Solving completed
27/03/2025 13:47:23 : Creating folder: C:\Users\promerogomb\Desktop\fluxcontrol\motores\PLACond\Emag\
27/03/2025 13:47:23 : Nodes count = 3365
27/03/2025 13:47:23 : Elements count = 6472
27/03/2025 13:47:23 : Status: Solving Completed
27/03/2025 13:47:23 : pymotorcad: ExportResults
27/03/2025 13:47:23 : pymotorcad: Quit
