Drive
"DC Bus Voltage";350;Volts;
"Line-Line Supply Voltage (rms)";247,5;Volts;
"Phase Supply Voltage (rms)";142,9;Volts;
"Line-Line Terminal Voltage (peak)";455,8;Volts;
"Line-Line Terminal Voltage (rms)";309,6;Volts;
"Phase Terminal Voltage (peak)";251,8;Volts;
"Phase Terminal Voltage (rms)";178,9;Volts;
"Harmonic Distortion Line-Line Terminal Voltage";6,585;%;
"Harmonic Distortion Phase Terminal Voltage";6,633;%;
"Back EMF Line-Line Voltage (peak)";508,9;Volts;
"Back EMF Phase Voltage (peak)";293,8;Volts;
"Back EMF Line-Line Voltage (rms)";359,9;Volts;
"Back EMF Phase Voltage (rms)";207,8;Volts;
"Max Line-Line / Phase Voltage Ratio";1,732;;
"DC Supply Current (mean)";4,413;Amps;
"Line Current (peak)";4,243;Amps;
"Line Current (rms)";3;Amps;
"Phase Current (peak)";4,243;Amps;
"Phase Current (rms)";3;Amps;
"Phase Advance";45;EDeg;
"Drive Offset Angle (Open Circuit)";390;EDeg;
"Drive Offset Angle (On load)";30;EDeg;
"Phase Advance to give maximum torque";4,547;EDeg;
"Phasor Offset Angle";330;EDeg;
"Phasor Angle (Ph1)";0;EDeg;
"Phasor Angle (Ph2)";120;EDeg;
"Phasor Angle (Ph3)";240;EDeg;
"Max Angle Between Phasors";120;EDeg;
"D Axis Inductance";16,25;mH;
"Q Axis Inductance";18,17;mH;
"Line-Line Inductance (DQ)";33,53;mH;
"Armature End Winding Inductance_(Rosa and Grover)";0,544;mH;
"D Axis Phase Current (average rms)";-2,121;Amps;
"Q Axis Phase Current (average rms)";2,121;Amps;
"Torque Constant (Kt)";1,026;Nm/A;
"Motor Constant (Km)";0,3278;Nm/(Watts^0.5);
"Back EMF Constant (Ke) (fundamental)";1,62;Vs/Rad;
"Electrical Constant";2,637;msec;
"Electrical Loading";5,003E004;Amps/m;
"Stall Current";26,82;Amps;
"Stall Torque";27,51;Nm;
"Short Circuit Line Current (peak)";9,95;Amps;
"Short Circuit Current Density (peak)";50,67;Amps/mm²;
"Short Circuit Current Density (rms)";35,83;Amps/mm²;
"Short Circuit Braking Torque";-3,084;Nm;
"Short Circuit Max Braking Torque";-7,207;Nm;
"Short Circuit Max Braking Torque Speed";678,4;rpm;
"Fundamental Frequency";300;Hz;
"Shaft Speed";3000;rpm;

E-Magnetics
"Maximum torque possible (DQ)_(For Phase Advance of 4,547 EDeg)";5,9709;Nm;
"Average torque (virtual work)";4,3593;Nm;
"Average torque (loop torque)";4,332;Nm;
"Torque Ripple (MsVw)";0,60512;Nm;
"Torque Ripple (MsVw) [%]";13,907;%;
"Speed limit for constant torque_(For Phase Advance of 45 EDeg)";2324,8;rpm;
"No load speed";2063,2;rpm;
"Speed limit for zero q axis current";INF;rpm;
"Electromagnetic Power_Operating point outside voltage limit.";1367;Watts;
"Input Power";1544,4;Watts;
"Total Losses (on load)";210,54;Watts;
"Output Power_Operating point outside voltage limit.";1333,9;Watts;
"System Efficiency";86,368;%;
"Shaft Torque";4,246;Nm;
"Power Factor [Waveform] (leading)";0,96066;;
"Power Factor Angle [Waveform]";-16,124;EDeg;
"Power Factor [THD]";0,95856;;
"Power Factor [Phasor] (leading)";0,96126;;
"Power Factor Angle [Phasor]";344;EDeg;
"Load Angle [Phasor]";28,908;EDeg;
"Phase Terminal Voltage (rms) [Phasor]";178,91;Volts;
"Rotor Inertia";0,00063702;kg.m²;
"Shaft Inertia";3,2257E-005;kg.m²;
"Total Inertia";0,00066928;kg.m²;
"Torque per rotor volume";40,307;kNm/m³;
"Rotor peripheral velocity (on load)";13,022;m/s;
"Flux Linkage D (Q axis current)";155,875;mVs;
"Flux Linkage Q (Q axis current)";54,453;mVs;
"Flux linkage D (On load)";107,122;mVs;
"Flux linkage Q (On load)";54,5023;mVs;
"Torque Constant (Kt)";1,0256;Nm/A;
"Motor Constant (Km)";0,327818;Nm/(Watts^0.5);
"Back EMF Constant (Ke) (fundamental)";1,6199;Vs/Rad;
"Stall Current";26,8188;Amps;
"Stall Torque";27,5053;Nm;
"Cogging Period";10;MDeg;
"Cogging Frequency";1800;Hz;
"Fundamental Frequency";300;Hz;
"Mechanical Frequency";50;Hz;
"Optimum Skewing Angle";10;MDeg;
"Magnetic Symmetry Factor_(Automatic calculation)";6;;
"Magnetic Axial Length (Slice1)";20;mm;

Phasor Diagram
"Maximum torque possible (DQ)_(For Phase Advance of 4,547 EDeg)";5,9709;Nm;
"Average torque (virtual work)";4,3593;Nm;
"Average torque (loop torque)";4,332;Nm;
"Torque Ripple (MsVw)";0,60512;Nm;
"Torque Ripple (MsVw) [%]";13,907;%;
"Speed limit for constant torque_(For Phase Advance of 45 EDeg)";2324,8;rpm;
"No load speed";2063,2;rpm;
"Speed limit for zero q axis current";INF;rpm;
"Electromagnetic Power_Operating point outside voltage limit.";1367;Watts;
"Input Power";1544,4;Watts;
"Total Losses (on load)";210,54;Watts;
"Output Power_Operating point outside voltage limit.";1333,9;Watts;
"System Efficiency";86,368;%;
"Shaft Torque";4,246;Nm;
"Power Factor [Waveform] (leading)";0,96066;;
"Power Factor Angle [Waveform]";-16,124;EDeg;
"Power Factor [THD]";0,95856;;
"Power Factor [Phasor] (leading)";0,96126;;
"Power Factor Angle [Phasor]";344;EDeg;
"Load Angle [Phasor]";28,908;EDeg;
"Phase Terminal Voltage (rms) [Phasor]";178,91;Volts;
"Rotor Inertia";0,00063702;kg.m²;
"Shaft Inertia";3,2257E-005;kg.m²;
"Total Inertia";0,00066928;kg.m²;
"Torque per rotor volume";40,307;kNm/m³;
"Rotor peripheral velocity (on load)";13,022;m/s;
"Flux Linkage D (Q axis current)";155,875;mVs;
"Flux Linkage Q (Q axis current)";54,453;mVs;
"Flux linkage D (On load)";107,122;mVs;
"Flux linkage Q (On load)";54,5023;mVs;
"Torque Constant (Kt)";1,0256;Nm/A;
"Motor Constant (Km)";0,327818;Nm/(Watts^0.5);
"Back EMF Constant (Ke) (fundamental)";1,6199;Vs/Rad;
"Stall Current";26,8188;Amps;
"Stall Torque";27,5053;Nm;
"Cogging Period";10;MDeg;
"Cogging Frequency";1800;Hz;
"Fundamental Frequency";300;Hz;
"Mechanical Frequency";50;Hz;
"Optimum Skewing Angle";10;MDeg;
"Magnetic Symmetry Factor_(Automatic calculation)";6;;
"Magnetic Axial Length (Slice1)";20;mm;

Equivalent Circuit
"Phase Resistance";6,525;Ohms;
"D Axis Inductance";16,25;mH;
"Q Axis Inductance";18,17;mH;
"Stator Slot Leakage Inductance";11,01;mH;
"Stator Differential Leakage Inductance";1,824;mH;
"Armature End Winding Inductance_(Rosa and Grover)";0,544;mH;
"Stator Leakage Inductance (Total)";13,37;mH;
"Magnetizing Inductance (D Axis)";2,876;mH;
"Magnetizing Inductance (Q Axis)";4,793;mH;
"D Axis Reactance";30,63;Ohms;
"Q Axis Reactance";34,24;Ohms;
"Stator Slot Leakage Reactance";20,75;Ohms;
"Stator Differential Leakage Reactance";3,438;Ohms;
"Armature End Winding Reactance";1,025;Ohms;
"Stator Leakage Reactance (Total)";25,21;Ohms;
"Magnetizing Reactance (D Axis)";5,422;Ohms;
"Magnetizing Reactance (Q Axis)";9,034;Ohms;
"Rotor Referred Resistance";183,8;Ohms;
"First Order Transient Reactance (D Axis)";25,21;Ohms;
"First Order Transient Reactance (Q Axis)";34,24;Ohms;
"Excitation Time Constant (Te)";1,565E-005;secs;
"First Order Transient Time Constant (Td')";1,288E-005;secs;
"Armature Time Constant (Ta)";0,002417;secs;

Flux Densities
"Airgap flux density (mean)";0,5647;Tesla;
"Airgap Flux Density (peak)";1,002;Tesla;
"Stator Tooth Flux Density (peak)";0,9435;Tesla;
"Stator Tooth Tip Flux Density (peak)";1,927;Tesla;
"Stator Back Iron Flux Density (peak)";1,343;Tesla;
"Rotor Back Iron Flux Density (peak)";0,3478;Tesla;

Losses
"Armature DC Copper Loss (on load)";176,2;Watts;
"Magnet Loss (on load)";0,6921;Watts;
"Stator iron Loss [total] (on load)";33,08;Watts;
"Rotor iron Loss [total] (on load)";0,5847;Watts;
"Windage Loss (user input)";0;Watts;
"Friction Loss (user input)";0;Watts;
"Shaft Loss [total] (on load)";0;Watts;
"Total Losses (on load)";210,5;Watts;
"Magnet Block Width";14,62;mm;
"Magnet Loss Factor";0,4889;;
"Magnet Loss (on load)";0,6921;Watts;
"Stator back iron Loss [hysteresis - fundamental] (on load)";2,964;Watts;
"Stator back iron Loss [hysteresis - minor loops] (on load)";2,236;Watts;
"Stator back iron Loss [hysteresis] (on load)";5,2;Watts;
"Stator back iron Loss [eddy] (on load)";6,664;Watts;
"Stator back iron Loss [excess] (on load)";0;Watts;
"Stator back iron Loss [total] (on load)";11,86;Watts;
"Stator tooth Loss [hysteresis - fundamental] (on load)";9,548;Watts;
"Stator tooth Loss [hysteresis - minor loops] (on load)";0,1072;Watts;
"Stator tooth Loss [hysteresis] (on load)";9,656;Watts;
"Stator tooth Loss [eddy] (on load)";11,56;Watts;
"Stator tooth Loss [excess] (on load)";0;Watts;
"Stator tooth Loss [total] (on load)";21,21;Watts;
"Stator iron Loss [total] (on load)";33,08;Watts;
"Rotor back iron Loss [hysteresis] (on load)";0;Watts;
"Rotor back iron Loss [eddy] (on load)";0,5847;Watts;
"Rotor back iron Loss [excess] (on load)";0;Watts;
"Rotor back iron Loss [total] (on load)";0,5847;Watts;
"Rotor iron Loss [total] (on load)";0,5847;Watts;
"Shaft Loss [eddy] (on load)";0;Watts;

Winding
"Armature Conductor CSA";0,1963;mm²;
"Armature Conductor Current Density";15,28;Amps/mm²;
"Armature Conductor MLT";74,23;mm;
"Armature Turns per Phase";750;;
"Armature Turns per Coil";125;;
"Length of phase";5,568E004;mm;
"Phase Resistance";6,525;Ohms;
"Line-Line Resistance";13,05;Ohms;
"Armature Conductor Temperature";106,7;°C;
"Mean Coil Pitch (Calculated)";19,25;mm;
"Mean Coil Pitch (Used)";9,624;mm;
"Fundamental Winding Factor";0,866;;
"Winding Factor Sum";0,09009;;
"Wire Ins Thickness";0,025;mm;
"Copper Diameter";0,5;mm;
Conductors/Slot;250;;
"Armature End Winding MLT (Calculated)";68,47;mm;
"Armature End Winding MLT (User adjustment)";0,5;;
"Armature End Winding MLT (Used)";34,23;mm;
"Copper Slot Fill (Wdg Area)";0,2523;;
"Wire Slot Fill (Slot Area)";0,2684;;
"Copper Slot Fill (Slot Area)";0,2218;;
"Heavy Build Slot Fill";0,3887;;
"Slot Area (Slot 1)";221,3;mm²;
"Winding Area (+ Liner) (Slot 1)";207,1;mm²;
"Slot Area (FEA)";207,1;mm²;
"Wedge Area";14,19;mm²;
"Slot Opening Area";1,598;mm²;
"Liner-Lam Gap Area (Slot 1)";0;mm²;
"Impreg Area (Slot 1)";135,2;mm²;
"Liner Area (Slot 1)";12,55;mm²;
"Coil Divider Area (Slot 1)";0;mm²;
"Volume Copper EWdg Front";5376;mm³;
"Volume Copper Active";1,767E004;mm³;
"Volume Copper EWdg Rear";5376;mm³;

Miscellaneous
"FEA Mesh Nodes";3365;;
"FEA Mesh Elements";6472;;
"Airgap Mesh Layers Used";5;;
"FEA Max Element Length";1,25;mm;

Materials
"Armature Conductor Resistivity";2,301E-008;Ohm.m;
"Armature Conductor Resistivity at Ref Temp (20°C)";1,724E-008;Ohm.m;
"Armature Conductor Temperature";106,7;°C;
"Stator Lamination Resistivity";2,3E-007;Ohm.m;
"Number of stator laminations";38,8;;
"Rotor Lamination Resistivity";1,43E-007;Ohm.m;
"Rotor Lamination Resistivity at Ref Temp (20°C)";1,43E-007;Ohm.m;
"Rotor Lamination Temperature";87,2;°C;
"Number of rotor laminations";1;;
"Shaft Resistivity";0;Ohm.m;
"Shaft Resistivity at Ref Temp (20°C)";0;Ohm.m;
"Shaft Temperature";85,57;°C;
"Magnet Resistivity";1,8E-006;Ohm.m;
"Magnet Resistivity at Ref Temp (20°C)";1,8E-006;Ohm.m;
"Magnet Temperature";87,67;°C;
"Total Motor Weight";2,646;kg;
"Weight Stator Lam";0,6688;kg;
"Armature Copper [Total] Weight";0,293;kg;
"Weight Rotor Lam";0,4923;kg;
"Weight Magnet";0,1315;kg;
"Weight Shaft Total";0,3224;kg;
"Magnet Br at reference temperature (20 °C)";1,26;Tesla;
"Magnet Temperature";87,67;°C;
"Magnet Br (Calculated)";1,158;Tesla;
"Magnet Br Adjustment Factor";1;;
"Magnet Br (Used)";1,158;Tesla;

